|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| SMPL\_SendOpt | nwk\_api.c |  |  |  |  |
|  | nwk\_getConnInfo | nwk.c |  |  |  |
|  | MRFI\_GetRadioState | mrfi\_radio.c |  |  |  |
|  | nwk\_checkConnInfo | nwk.c |  |  |  |
|  | nwk\_buildFrame | nwk\_frame.c |  |  |  |
|  | nwk\_buildAckReqFrame | nwk\_frame.c | APP\_AUTO\_ACK |  |  |
|  | nwk\_setSecureFrame | nwk\_security.c | SMPL\_SECURE |  |  |
|  | nwk\_isSandFClient | nwk\_join.c | ACCESS\_POINT |  |  |
|  | nwk\_sendFrame | nwk\_frame.c |  |  |  |
|  | NWK\_CHECK\_FOR\_SETRX | nwk\_types.h | APP\_AUTO\_ACK |  |  |
|  | NWK\_REPLY\_DELAY | nwk\_types.h | APP\_AUTO\_ACK |  |  |
|  | NWK\_CHECK\_FOR\_RESTORE\_STATE | nwk\_types.h | APP\_AUTO\_ACK |  |  |
|  |  |  |  |  |  |